

**How to measure for roof lantern blinds**

When **measuring for roof lantern blinds** the first thing you need to do is to decide where in the recess you are going to fit the blind. This location depends a lot on your particular circumstance eg how deep is your recess? Also some of our products are only suitable for installation at certain points in a recess.

[**SkyFIT™ Manual Blind**](https://blog.skylight-blinds-direct.co.uk/products/skyfit-manual/) : Must be fitted at the bottom edge of the recess (flush with the ceiling)

[**SkyFIT™ Motorised Blind**](https://blog.skylight-blinds-direct.co.uk/products/skyfit-motorised/): Can be fitted anywhere in the recess

[**LanternLITE™ Honeycomb blinds (including OPENVIEW**](https://blog.skylight-blinds-direct.co.uk/products/honeycomb-openview/)): Can be fitted anywhere in the recess

[**LanternLITE™ Zip & Twin Zip Blinds**](https://blog.skylight-blinds-direct.co.uk/products/zip-twin-zip/): Must be fitted at least 10cm up from the bottom of the recess

1. **Decide Where in the recess to Fit your Blind**
2. **Mark with a pencil**
3. **Measure the width & length in 3 places making no deductions (wall to wall – this is the RECESS SIZE).**

|  |  |
| --- | --- |
| Chart, radar chart  Description automatically generated | Chart, radar chart  Description automatically generated |

